T35A0 293:501 SEGGER J-Link V6.46 Log File (0000ms, 13073ms total)
T35A0 293:501 DLL Compiled: May 23 2019 17:49:56 (0000ms, 13073ms total)
T35A0 293:501 Logging started @ 2023-08-26 13:40 (0000ms, 13073ms total)
T35A0 293:501 JLINK_SetWarnOutHandler(...) (0000ms, 13073ms total)
T35A0 293:501 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled May  7 2021 16:26:12
Hardware: V9.40
S/N: 69406807
Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
TELNET listener socket opened on port 19021WEBSRV 
Starting webserver (0028ms, 13101ms total)
T35A0 293:501 WEBSRV Webserver running on local port 19080 (0028ms, 13101ms total)
T35A0 293:501   returns O.K. (0028ms, 13101ms total)
T35A0 293:530 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 13101ms total)
T35A0 293:530 JLINK_TIF_GetAvailable(...) (0000ms, 13101ms total)
T35A0 293:530 JLINK_SetErrorOutHandler(...) (0000ms, 13101ms total)
T35A0 293:530 JLINK_ExecCommand("ProjectFile = "D:\Project\Lora_gateway_sx1278\app\MDKProject\JLinkSettings.ini"", ...).   returns 0x00 (0001ms, 13102ms total)
T35A0 293:531 JLINK_ExecCommand("Device = STM32F207ZGTx", ...). Device "STM32F207ZG" selected.  returns 0x00 (0001ms, 13103ms total)
T35A0 293:532 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetDLLVersion()  returns 64600 (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetFirmwareString(...) (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetDLLVersion()  returns 64600 (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetCompileDateTime() (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetFirmwareString(...) (0000ms, 13103ms total)
T35A0 293:532 JLINK_GetHardwareVersion()  returns 0x16F30 (0000ms, 13103ms total)
T35A0 293:532 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0002ms, 13105ms total)
T35A0 293:534 JLINK_SetSpeed(500) (0000ms, 13105ms total)
T35A0 293:534 JLINK_GetId() >0x10B TIF>Found SW-DP with ID 0x2BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>
 >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x10B TIF>Found SW-DP with ID 0x2BA01477 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF>Scanning AP map to find all available APs >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>
AP[1]: Stopped AP scan as end of AP map has been reachedAP[0]: AHB-AP (IDR: 0x24770011)Iterating through AP map to find AHB-AP to use >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF> >0x42 TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>AP[0]: Core foundAP[0]: AHB-AP ROM base: 0xE00FF000 >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x28 TIF> >0x0D TIF> >0x21 TIF> >0x0D TIF> >0x21 TIF>
CPUID register: 0x412FC230. Implementer code: 0x41 (ARM)Found Cortex-M3 r2p0, Little endian. -- Max. mem block: 0x00011028 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE0002000)FPUnit: 6 code (BP) slots and 2 literal slots -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000) -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)
 -- CPU_ReadMem(4 bytes @ 0xE000ED88) -- CPU_WriteMem(4 bytes @ 0xE000ED88)CoreSight components:ROMTbl[0] @ E00FF000 -- CPU_ReadMem(16 bytes @ 0xE00FF000) -- CPU_ReadMem(16 bytes @ 0xE000EFF0) -- CPU_ReadMem(16 bytes @ 0xE000EFE0)ROMTbl[0][0]: E000E000, CID: B105E00D, PID: 002BB000 SCS -- CPU_ReadMem(16 bytes @ 0xE0001FF0) -- CPU_ReadMem(16 bytes @ 0xE0001FE0)ROMTbl[0][1]: E0001000, CID: B105E00D, PID: 002BB002 DWT -- CPU_ReadMem(16 bytes @ 0xE0002FF0) -- CPU_ReadMem(16 bytes @ 0xE0002FE0)
ROMTbl[0][2]: E0002000, CID: B105E00D, PID: 002BB003 FPB -- CPU_ReadMem(16 bytes @ 0xE0000FF0) -- CPU_ReadMem(16 bytes @ 0xE0000FE0)ROMTbl[0][3]: E0000000, CID: B105E00D, PID: 002BB001 ITM -- CPU_ReadMem(16 bytes @ 0xE00FF010) -- CPU_ReadMem(16 bytes @ 0xE0040FF0) -- CPU_ReadMem(16 bytes @ 0xE0040FE0)ROMTbl[0][4]: E0040000, CID: B105900D, PID: 002BB923 TPIU-Lite -- CPU_ReadMem(16 bytes @ 0xE0041FF0) -- CPU_ReadMem(16 bytes @ 0xE0041FE0)ROMTbl[0][5]: E0041000, CID: B105900D, PID: 002BB924 ETM-M3
 >0x0D TIF> >0x21 TIF>  returns 0x2BA01477 (0190ms, 13295ms total)
T35A0 293:724 JLINK_GetDLLVersion()  returns 64600 (0000ms, 13295ms total)
T35A0 293:724 JLINK_CORE_GetFound()  returns 0x30000FF (0000ms, 13295ms total)
T35A0 293:724 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 13295ms total)
T35A0 293:724 JLINK_GetDebugInfo(0x100 = JLINKARM_ROM_TABLE_ADDR_INDEX) -- Value=0xE00FF000  returns 0x00 (0000ms, 13295ms total)
T35A0 293:724 JLINK_GetDebugInfo(0x101 = JLINKARM_DEBUG_INFO_ETM_ADDR_INDEX) -- Value=0xE0041000  returns 0x00 (0000ms, 13295ms total)
T35A0 293:724 JLINK_ReadMemEx(0xE0041FD0, 0x0020 Bytes, ..., Flags = 0x02000004) -- CPU_ReadMem(32 bytes @ 0xE0041FD0) - Data: 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...  returns 0x20 (0002ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x102 = JLINKARM_DEBUG_INFO_MTB_ADDR_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x103 = JLINKARM_DEBUG_INFO_TPIU_ADDR_INDEX) -- Value=0xE0040000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x104 = JLINKARM_DEBUG_INFO_ITM_ADDR_INDEX) -- Value=0xE0000000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x105 = JLINKARM_DEBUG_INFO_DWT_ADDR_INDEX) -- Value=0xE0001000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x106 = JLINKARM_DEBUG_INFO_FPB_ADDR_INDEX) -- Value=0xE0002000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x107 = JLINKARM_DEBUG_INFO_NVIC_ADDR_INDEX) -- Value=0xE000E000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x10C = JLINKARM_DEBUG_INFO_DBG_ADDR_INDEX) -- Value=0xE000EDF0  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_GetDebugInfo(0x01 = Unknown) -- Value=0x00000000  returns 0x00 (0000ms, 13297ms total)
T35A0 293:726 JLINK_ReadMemU32(0xE000ED00, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED00) - Data: 30 C2 2F 41  returns 1 (0002ms, 13299ms total)
T35A0 293:728 JLINK_GetDebugInfo(0x10F = JLINKARM_DEBUG_INFO_HAS_CORTEX_M_SECURITY_EXT_INDEX) -- Value=0x00000000  returns 0x00 (0000ms, 13299ms total)
T35A0 293:728 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 13299ms total)
T35A0 293:728 JLINK_Reset() -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU is running -- CPU_WriteMem(4 bytes @ 0xE000EDFC)
 -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0097ms, 13396ms total)
T35A0 293:825 JLINK_ReadReg(R15 (PC))  returns 0x08000198 (0000ms, 13396ms total)
T35A0 293:825 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 13396ms total)
T35A0 293:825 JLINK_Halt()  returns 0x00 (0000ms, 13396ms total)
T35A0 293:825 JLINK_ReadMemU32(0xE000EDF0, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) - Data: 03 00 03 00  returns 1 (0002ms, 13398ms total)
T35A0 293:827 JLINK_WriteU32(0xE000EDF0, 0xA05F0003) -- CPU_WriteMem(4 bytes @ 0xE000EDF0)  returns 0 (0001ms, 13399ms total)
T35A0 293:828 JLINK_WriteU32(0xE000EDFC, 0x01000000) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)  returns 0 (0001ms, 13400ms total)
T35A0 293:829 JLINK_GetHWStatus(...)  returns 0x00 (0000ms, 13400ms total)
T35A0 293:829 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)  returns 0x06 (0000ms, 13400ms total)
T35A0 293:829 JLINK_GetNumBPUnits(Type = 0xF0)  returns 0x2000 (0000ms, 13400ms total)
T35A0 293:829 JLINK_GetNumWPUnits()  returns 0x04 (0000ms, 13400ms total)
T35A0 293:829 JLINK_GetSpeed()  returns 0x1F4 (0000ms, 13400ms total)
T35A0 293:829 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0001ms, 13401ms total)
T35A0 293:830 JLINK_ReadMemU32(0xE000E004, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000E004) - Data: 02 00 00 00  returns 1 (0002ms, 13403ms total)
T35A0 293:832 JLINK_WriteMemEx(0xE0001000, 0x001C Bytes, ..., Flags = 0x02000004) - Data: 01 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ... -- CPU_WriteMem(28 bytes @ 0xE0001000)  returns 0x1C (0003ms, 13406ms total)
T35A0 293:835 JLINK_ReadReg(R15 (PC))  returns 0x08000198 (0000ms, 13406ms total)
T35A0 293:835 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 13406ms total)
T35A0 293:840 JLINK_ReadMemEx(0xE0001004, 0x0004 Bytes, ..., Flags = 0x02000000) - Data: 00 00 00 00  returns 0x04 (0000ms, 13406ms total)
T35A0 293:921 JLINK_SetResetType(JLINKARM_CM3_RESET_TYPE_NORMAL)  returns JLINKARM_CM3_RESET_TYPE_NORMAL (0000ms, 13406ms total)
T35A0 293:921 JLINK_Reset() -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC)Reset: Halt core after reset via DEMCR.VC_CORERESET. >0x35 TIF>Reset: Reset device via AIRCR.SYSRESETREQ. -- CPU_WriteMem(4 bytes @ 0xE000ED0C) >0x0D TIF> >0x28 TIF> -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE000EDF0) -- CPU_WriteMem(4 bytes @ 0xE0002000)
 -- CPU_ReadMem(4 bytes @ 0xE000EDFC) -- CPU_ReadMem(4 bytes @ 0xE0001000) (0092ms, 13498ms total)
T35A0 294:013 JLINK_ReadReg(R15 (PC))  returns 0x08000198 (0000ms, 13498ms total)
T35A0 294:013 JLINK_ReadReg(XPSR)  returns 0x01000000 (0000ms, 13498ms total)
T35A0 294:122 JLINK_ReadMemEx(0x08000198, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x08000180) -- Updating C cache (128 bytes @ 0x08000180) -- Read from C cache (60 bytes @ 0x08000198) - Data: 06 48 80 47 06 48 00 47 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0006ms, 13504ms total)
T35A0 294:128 JLINK_ReadMemEx(0x08000198, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08000198) - Data: 06 48  returns 0x02 (0000ms, 13504ms total)
T35A0 294:128 JLINK_ReadMemEx(0x0800019A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x0800019A) - Data: 80 47  returns 0x02 (0000ms, 13504ms total)
T35A0 294:128 JLINK_ReadMemEx(0x0800019A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x0800019A) - Data: 80 47  returns 0x02 (0000ms, 13504ms total)
T35A0 294:128 JLINK_ReadMemEx(0x0800019C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x0800019C) - Data: 06 48 00 47 FE E7 FE E7 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0000ms, 13504ms total)
T35A0 294:128 JLINK_ReadMemEx(0x0800019C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x0800019C) - Data: 06 48  returns 0x02 (0000ms, 13504ms total)
T35A0 294:851 JLINK_ReadMemEx(0x0800019C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x0800019C) - Data: 06 48 00 47 FE E7 FE E7 FE E7 FE E7 FE E7 FE E7 ...  returns 0x3C (0000ms, 13504ms total)
T35A0 294:851 JLINK_ReadMemEx(0x0800019C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x0800019C) - Data: 06 48  returns 0x02 (0000ms, 13504ms total)
T35A0 294:851 JLINK_ReadMemEx(0x0800019E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x0800019E) - Data: 00 47  returns 0x02 (0000ms, 13504ms total)
T5634 295:009 JLINK_ReadMemEx(0x08000198, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08000198) - Data: 06 48  returns 0x02 (0000ms, 13504ms total)
T5634 295:009 JLINK_SetBPEx(Addr = 0x08009F70, Type = 0xFFFFFFF2)  returns 0x00000001 (0000ms, 13504ms total)
T5634 295:009 JLINK_Go() -- CPU_WriteMem(4 bytes @ 0xE0002000) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_WriteMem(4 bytes @ 0xE000200C) -- CPU_WriteMem(4 bytes @ 0xE0002010) -- CPU_WriteMem(4 bytes @ 0xE0002014) -- CPU_WriteMem(4 bytes @ 0xE0002018) -- CPU_WriteMem(4 bytes @ 0xE000201C) -- CPU_WriteMem(4 bytes @ 0xE0001004) (0013ms, 13517ms total)
T5634 295:124 JLINK_IsHalted()  returns TRUE (0016ms, 13533ms total)
T5634 295:140 JLINK_Halt()  returns 0x00 (0000ms, 13517ms total)
T5634 295:140 JLINK_IsHalted()  returns TRUE (0000ms, 13517ms total)
T5634 295:140 JLINK_IsHalted()  returns TRUE (0000ms, 13517ms total)
T5634 295:140 JLINK_IsHalted()  returns TRUE (0000ms, 13517ms total)
T5634 295:140 JLINK_ReadReg(R15 (PC))  returns 0x08009F70 (0000ms, 13517ms total)
T5634 295:140 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 13517ms total)
T5634 295:140 JLINK_ClrBPEx(BPHandle = 0x00000001)  returns 0x00 (0000ms, 13517ms total)
T5634 295:140 JLINK_ReadMemU32(0xE000ED30, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE000ED30) - Data: 02 00 00 00  returns 1 (0001ms, 13518ms total)
T5634 295:141 JLINK_ReadMemU32(0xE0001028, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001028) - Data: 00 00 00 00  returns 1 (0001ms, 13519ms total)
T5634 295:142 JLINK_ReadMemU32(0xE0001038, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001038) - Data: 00 02 00 00  returns 1 (0001ms, 13520ms total)
T5634 295:143 JLINK_ReadMemU32(0xE0001048, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001048) - Data: 00 00 00 00  returns 1 (0002ms, 13522ms total)
T5634 295:145 JLINK_ReadMemU32(0xE0001058, 0x0001 Items, ...) -- CPU_ReadMem(4 bytes @ 0xE0001058) - Data: 00 00 00 00  returns 1 (0001ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R0)  returns 0x08009F71 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R1)  returns 0x2001B2E0 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R2)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R3)  returns 0x08006265 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R4)  returns 0x08036B2C (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R5)  returns 0x08036B2C (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R6)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R7)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R8)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R9)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R10)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R11)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R12)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R13 (SP))  returns 0x2001B2E0 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R14)  returns 0x08000EDD (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(R15 (PC))  returns 0x08009F70 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(XPSR)  returns 0x61000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(MSP)  returns 0x2001B2E0 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(PSP)  returns 0x00000000 (0000ms, 13523ms total)
T5634 295:146 JLINK_ReadReg(CFBP)  returns 0x00000000 (0000ms, 13523ms total)
T35A0 295:247 JLINK_ReadMemEx(0x08009E70, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(128 bytes @ 0x08009E40) -- Updating C cache (128 bytes @ 0x08009E40) -- Read from C cache (60 bytes @ 0x08009E70) - Data: 41 00 0D 4C 04 EB 80 00 40 89 08 B1 00 20 DC E7 ...  returns 0x3C (0005ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E70, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E70) - Data: 41 00  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E72, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E72) - Data: 0D 4C  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E72, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E72) - Data: 0D 4C  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E74, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E74) - Data: 04 EB 80 00 40 89 08 B1 00 20 DC E7 13 B1 4F F4 ...  returns 0x3C (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E74, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E74) - Data: 04 EB  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E74, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E74) - Data: 04 EB 80 00 40 89 08 B1 00 20 DC E7 13 B1 4F F4 ...  returns 0x3C (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E74, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E74) - Data: 04 EB  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E76, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E76) - Data: 80 00  returns 0x02 (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E78, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E78) - Data: 40 89 08 B1 00 20 DC E7 13 B1 4F F4 80 70 06 E0 ...  returns 0x3C (0000ms, 13528ms total)
T35A0 295:252 JLINK_ReadMemEx(0x08009E78, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E78) - Data: 40 89  returns 0x02 (0001ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7A) - Data: 08 B1  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7A) - Data: 08 B1  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E7C) - Data: 00 20 DC E7 13 B1 4F F4 80 70 06 E0 01 EB 41 00 ...  returns 0x3C (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7C) - Data: 00 20  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E7C) - Data: 00 20 DC E7 13 B1 4F F4 80 70 06 E0 01 EB 41 00 ...  returns 0x3C (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7C) - Data: 00 20  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7E) - Data: DC E7  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E7E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E7E) - Data: DC E7  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E80, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E80) - Data: 13 B1 4F F4 80 70 06 E0 01 EB 41 00 06 4C 04 EB ...  returns 0x3C (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E80, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E80) - Data: 13 B1  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E80, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E80) - Data: 13 B1 4F F4 80 70 06 E0 01 EB 41 00 06 4C 04 EB ...  returns 0x3C (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E80, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E80) - Data: 13 B1  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E82, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E82) - Data: 4F F4  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E82, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E82) - Data: 4F F4  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E84, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E84) - Data: 80 70 06 E0 01 EB 41 00 06 4C 04 EB 80 00 40 89 ...  returns 0x3C (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E84, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E84) - Data: 80 70  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E86, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E86) - Data: 06 E0  returns 0x02 (0000ms, 13529ms total)
T35A0 295:253 JLINK_ReadMemEx(0x08009E88, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08009EC0) -- Updating C cache (64 bytes @ 0x08009EC0) -- Read from C cache (60 bytes @ 0x08009E88) - Data: 01 EB 41 00 06 4C 04 EB 80 00 40 89 40 1C 01 EB ...  returns 0x3C (0003ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E88, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E88) - Data: 01 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E88, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E88) - Data: 01 EB 41 00 06 4C 04 EB 80 00 40 89 40 1C 01 EB ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E88, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E88) - Data: 01 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E8A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E8A) - Data: 41 00  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E8C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E8C) - Data: 06 4C 04 EB 80 00 40 89 40 1C 01 EB 41 04 03 4D ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E8C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E8C) - Data: 06 4C  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E8E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E8E) - Data: 04 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E8E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E8E) - Data: 04 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E90, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E90) - Data: 80 00 40 89 40 1C 01 EB 41 04 03 4D 05 EB 84 04 ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E90, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E90) - Data: 80 00  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E92, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E92) - Data: 40 89  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E94, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E94) - Data: 40 1C 01 EB 41 04 03 4D 05 EB 84 04 60 81 48 1C ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E94, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E94) - Data: 40 1C  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E94, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E94) - Data: 40 1C 01 EB 41 04 03 4D 05 EB 84 04 60 81 48 1C ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E94, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E94) - Data: 40 1C  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E96, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E96) - Data: 01 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E96, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E96) - Data: 01 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E98, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E98) - Data: 41 04 03 4D 05 EB 84 04 60 81 48 1C C9 E7 00 00 ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E98, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E98) - Data: 41 04  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E9A) - Data: 03 4D  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E9C) - Data: 05 EB 84 04 60 81 48 1C C9 E7 00 00 2C 0D 01 20 ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E9C) - Data: 05 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009E9C) - Data: 05 EB 84 04 60 81 48 1C C9 E7 00 00 2C 0D 01 20 ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E9C) - Data: 05 EB  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009E9E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009E9E) - Data: 84 04  returns 0x02 (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009EA0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EA0) - Data: 60 81 48 1C C9 E7 00 00 2C 0D 01 20 2D E9 F0 41 ...  returns 0x3C (0000ms, 13532ms total)
T35A0 295:256 JLINK_ReadMemEx(0x08009EA0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA0) - Data: 60 81  returns 0x02 (0001ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA2) - Data: 48 1C  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA2) - Data: 48 1C  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EA4) - Data: C9 E7 00 00 2C 0D 01 20 2D E9 F0 41 04 46 0F 46 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA4) - Data: C9 E7  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EA4) - Data: C9 E7 00 00 2C 0D 01 20 2D E9 F0 41 04 46 0F 46 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA4) - Data: C9 E7  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EA6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EA6) - Data: 00 00  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EAC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EAC) - Data: 2D E9 F0 41 04 46 0F 46 15 46 1E 46 60 19 32 46 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EAC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EAC) - Data: 2D E9  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EAE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EAE) - Data: F0 41  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EB0) - Data: 04 46 0F 46 15 46 1E 46 60 19 32 46 39 46 F6 F7 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB0) - Data: 04 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB2) - Data: 0F 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB2) - Data: 0F 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EB4) - Data: 15 46 1E 46 60 19 32 46 39 46 F6 F7 06 FA BD E8 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB4) - Data: 15 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EB4) - Data: 15 46 1E 46 60 19 32 46 39 46 F6 F7 06 FA BD E8 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB4) - Data: 15 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB6) - Data: 1E 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB6) - Data: 1E 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EB8) - Data: 60 19 32 46 39 46 F6 F7 06 FA BD E8 F0 81 00 00 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB8) - Data: 60 19  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EB8) - Data: 60 19 32 46 39 46 F6 F7 06 FA BD E8 F0 81 00 00 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EB8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EB8) - Data: 60 19  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBA) - Data: 32 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBA) - Data: 32 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EBC) - Data: 39 46 F6 F7 06 FA BD E8 F0 81 00 00 2D E9 F0 41 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBC) - Data: 39 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EBC) - Data: 39 46 F6 F7 06 FA BD E8 F0 81 00 00 2D E9 F0 41 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBC) - Data: 39 46  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBE) - Data: F6 F7  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EBE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EBE) - Data: F6 F7  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EC0) - Data: 06 FA BD E8 F0 81 00 00 2D E9 F0 41 0B 30 20 F0 ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC0) - Data: 06 FA  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC2) - Data: BD E8  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EC4) - Data: F0 81 00 00 2D E9 F0 41 0B 30 20 F0 07 06 10 4D ...  returns 0x3C (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC4) - Data: F0 81  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC6) - Data: 00 00  returns 0x02 (0000ms, 13533ms total)
T35A0 295:257 JLINK_ReadMemEx(0x08009EC8, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08009F00) -- Updating C cache (64 bytes @ 0x08009F00) -- Read from C cache (60 bytes @ 0x08009EC8) - Data: 2D E9 F0 41 0B 30 20 F0 07 06 10 4D 19 E0 20 68 ...  returns 0x3C (0003ms, 13536ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EC8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC8) - Data: 2D E9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EC8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EC8) - Data: 2D E9 F0 41 0B 30 20 F0 07 06 10 4D 19 E0 20 68 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EC8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EC8) - Data: 2D E9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ECA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ECA) - Data: F0 41  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ECC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ECC) - Data: 0B 30 20 F0 07 06 10 4D 19 E0 20 68 B0 42 15 D3 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ECC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ECC) - Data: 0B 30  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ECE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ECE) - Data: 20 F0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ECE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ECE) - Data: 20 F0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ED0) - Data: 07 06 10 4D 19 E0 20 68 B0 42 15 D3 B0 42 0A D9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED0) - Data: 07 06  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED2) - Data: 10 4D  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ED4) - Data: 19 E0 20 68 B0 42 15 D3 B0 42 0A D9 87 1B 20 1D ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED4) - Data: 19 E0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ED4) - Data: 19 E0 20 68 B0 42 15 D3 B0 42 0A D9 87 1B 20 1D ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED4) - Data: 19 E0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED6) - Data: 20 68  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED6) - Data: 20 68  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ED8) - Data: B0 42 15 D3 B0 42 0A D9 87 1B 20 1D D4 F8 04 80 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED8) - Data: B0 42  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009ED8) - Data: B0 42 15 D3 B0 42 0A D9 87 1B 20 1D D4 F8 04 80 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009ED8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009ED8) - Data: B0 42  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDA) - Data: 15 D3  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDA) - Data: 15 D3  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EDC) - Data: B0 42 0A D9 87 1B 20 1D D4 F8 04 80 F6 F7 F1 F9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDC) - Data: B0 42  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EDC) - Data: B0 42 0A D9 87 1B 20 1D D4 F8 04 80 F6 F7 F1 F9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDC) - Data: B0 42  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDE) - Data: 0A D9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EDE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EDE) - Data: 0A D9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EE0) - Data: 87 1B 20 1D D4 F8 04 80 F6 F7 F1 F9 A0 19 C0 E9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE0) - Data: 87 1B  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EE0) - Data: 87 1B 20 1D D4 F8 04 80 F6 F7 F1 F9 A0 19 C0 E9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE0) - Data: 87 1B  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE2) - Data: 20 1D  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE2) - Data: 20 1D  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EE4) - Data: D4 F8 04 80 F6 F7 F1 F9 A0 19 C0 E9 00 78 28 60 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE4) - Data: D4 F8  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EE4) - Data: D4 F8 04 80 F6 F7 F1 F9 A0 19 C0 E9 00 78 28 60 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE4) - Data: D4 F8  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE6) - Data: 04 80  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EE8) - Data: F6 F7 F1 F9 A0 19 C0 E9 00 78 28 60 04 E0 60 68 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EE8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EE8) - Data: F6 F7  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EEA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EEA) - Data: F1 F9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EEC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EEC) - Data: A0 19 C0 E9 00 78 28 60 04 E0 60 68 28 60 20 1D ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EEC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EEC) - Data: A0 19  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EEE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EEE) - Data: C0 E9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EEE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EEE) - Data: C0 E9  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF0, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EF0) - Data: 00 78 28 60 04 E0 60 68 28 60 20 1D F6 F7 E7 F9 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF0, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF0) - Data: 00 78  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF2, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF2) - Data: 28 60  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EF4) - Data: 04 E0 60 68 28 60 20 1D F6 F7 E7 F9 20 1D 26 60 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF4) - Data: 04 E0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF4, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EF4) - Data: 04 E0 60 68 28 60 20 1D F6 F7 E7 F9 20 1D 26 60 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF4, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF4) - Data: 04 E0  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF6) - Data: 60 68  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF6, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF6) - Data: 60 68  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EF8) - Data: 28 60 20 1D F6 F7 E7 F9 20 1D 26 60 BD E8 F0 81 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF8) - Data: 28 60  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF8, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EF8) - Data: 28 60 20 1D F6 F7 E7 F9 20 1D 26 60 BD E8 F0 81 ...  returns 0x3C (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EF8, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EF8) - Data: 28 60  returns 0x02 (0000ms, 13537ms total)
T35A0 295:261 JLINK_ReadMemEx(0x08009EFA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EFA) - Data: 20 1D  returns 0x02 (0001ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFA, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EFA) - Data: 20 1D  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EFC) - Data: F6 F7 E7 F9 20 1D 26 60 BD E8 F0 81 25 1D 2C 68 ...  returns 0x3C (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EFC) - Data: F6 F7  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFC, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009EFC) - Data: F6 F7 E7 F9 20 1D 26 60 BD E8 F0 81 25 1D 2C 68 ...  returns 0x3C (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFC, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EFC) - Data: F6 F7  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009EFE, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009EFE) - Data: E7 F9  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F00, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F00) - Data: 20 1D 26 60 BD E8 F0 81 25 1D 2C 68 00 2C E2 D1 ...  returns 0x3C (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F00, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F00) - Data: 20 1D  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F02, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F02) - Data: 26 60  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F02, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F02) - Data: 26 60  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F04, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F04) - Data: BD E8 F0 81 25 1D 2C 68 00 2C E2 D1 00 20 F7 E7 ...  returns 0x3C (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F04, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F04) - Data: BD E8  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F04, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F04) - Data: BD E8 F0 81 25 1D 2C 68 00 2C E2 D1 00 20 F7 E7 ...  returns 0x3C (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F04, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F04) - Data: BD E8  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F06, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F06) - Data: F0 81  returns 0x02 (0000ms, 13538ms total)
T35A0 295:262 JLINK_ReadMemEx(0x08009F08, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08009F40) -- Updating C cache (64 bytes @ 0x08009F40) -- Read from C cache (60 bytes @ 0x08009F08) - Data: 25 1D 2C 68 00 2C E2 D1 00 20 F7 E7 B8 01 00 20 ...  returns 0x3C (0003ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F08, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F08) - Data: 25 1D  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0A) - Data: 2C 68  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0A) - Data: 2C 68  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F0C) - Data: 00 2C E2 D1 00 20 F7 E7 B8 01 00 20 10 B5 02 46 ...  returns 0x3C (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0C) - Data: 00 2C  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F0C) - Data: 00 2C E2 D1 00 20 F7 E7 B8 01 00 20 10 B5 02 46 ...  returns 0x3C (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0C) - Data: 00 2C  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0E) - Data: E2 D1  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F0E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F0E) - Data: E2 D1  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F10, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F10) - Data: 00 20 F7 E7 B8 01 00 20 10 B5 02 46 8C 7E CB 7E ...  returns 0x3C (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F10, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F10) - Data: 00 20  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F10, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F10) - Data: 00 20 F7 E7 B8 01 00 20 10 B5 02 46 8C 7E CB 7E ...  returns 0x3C (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F10, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F10) - Data: 00 20  returns 0x02 (0000ms, 13541ms total)
T35A0 295:265 JLINK_ReadMemEx(0x08009F12, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F12) - Data: F7 E7  returns 0x02 (0001ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F12, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F12) - Data: F7 E7  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F14, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F14) - Data: B8 01 00 20 10 B5 02 46 8C 7E CB 7E 44 EA 03 20 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F14, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F14) - Data: B8 01  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F18, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F18) - Data: 10 B5 02 46 8C 7E CB 7E 44 EA 03 20 13 78 03 2B ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F18, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F18) - Data: 10 B5  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1A) - Data: 02 46  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1A) - Data: 02 46  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F1C) - Data: 8C 7E CB 7E 44 EA 03 20 13 78 03 2B 05 D1 0C 7D ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1C) - Data: 8C 7E  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F1C) - Data: 8C 7E CB 7E 44 EA 03 20 13 78 03 2B 05 D1 0C 7D ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1C) - Data: 8C 7E  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1E) - Data: CB 7E  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F1E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F1E) - Data: CB 7E  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F20, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F20) - Data: 44 EA 03 20 13 78 03 2B 05 D1 0C 7D 4B 7D 44 EA ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F20, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F20) - Data: 44 EA  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F20, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F20) - Data: 44 EA 03 20 13 78 03 2B 05 D1 0C 7D 4B 7D 44 EA ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F20, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F20) - Data: 44 EA  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F22, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F22) - Data: 03 20  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F24, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F24) - Data: 13 78 03 2B 05 D1 0C 7D 4B 7D 44 EA 03 23 40 EA ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F24, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F24) - Data: 13 78  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F26, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F26) - Data: 03 2B  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F26, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F26) - Data: 03 2B  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F28, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F28) - Data: 05 D1 0C 7D 4B 7D 44 EA 03 23 40 EA 03 40 10 BD ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F28, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F28) - Data: 05 D1  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F28, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F28) - Data: 05 D1 0C 7D 4B 7D 44 EA 03 23 40 EA 03 40 10 BD ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F28, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F28) - Data: 05 D1  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2A) - Data: 0C 7D  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2A) - Data: 0C 7D  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F2C) - Data: 4B 7D 44 EA 03 23 40 EA 03 40 10 BD 00 BF 15 E0 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2C) - Data: 4B 7D  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F2C) - Data: 4B 7D 44 EA 03 23 40 EA 03 40 10 BD 00 BF 15 E0 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2C) - Data: 4B 7D  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2E) - Data: 44 EA  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F2E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F2E) - Data: 44 EA  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F30, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F30) - Data: 03 23 40 EA 03 40 10 BD 00 BF 15 E0 40 21 0B 48 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F30, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F30) - Data: 03 23  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F32, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F32) - Data: 40 EA  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F34, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F34) - Data: 03 40 10 BD 00 BF 15 E0 40 21 0B 48 F7 F7 8F FF ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F34, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F34) - Data: 03 40  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F36, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F36) - Data: 10 BD  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F38, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F38) - Data: 00 BF 15 E0 40 21 0B 48 F7 F7 8F FF 4F F4 FA 73 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F38, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F38) - Data: 00 BF  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F38, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F38) - Data: 00 BF 15 E0 40 21 0B 48 F7 F7 8F FF 4F F4 FA 73 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F38, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F38) - Data: 00 BF  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3A) - Data: 15 E0  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3A) - Data: 15 E0  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F3C) - Data: 40 21 0B 48 F7 F7 8F FF 4F F4 FA 73 00 22 11 46 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3C) - Data: 40 21  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F3C) - Data: 40 21 0B 48 F7 F7 8F FF 4F F4 FA 73 00 22 11 46 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3C) - Data: 40 21  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3E) - Data: 0B 48  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F3E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F3E) - Data: 0B 48  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F40, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F40) - Data: F7 F7 8F FF 4F F4 FA 73 00 22 11 46 10 46 F9 F7 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F40, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F40) - Data: F7 F7  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F40, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F40) - Data: F7 F7 8F FF 4F F4 FA 73 00 22 11 46 10 46 F9 F7 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F40, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F40) - Data: F7 F7  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F42, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F42) - Data: 8F FF  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F44, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F44) - Data: 4F F4 FA 73 00 22 11 46 10 46 F9 F7 8D F8 40 21 ...  returns 0x3C (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F44, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F44) - Data: 4F F4  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F46, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F46) - Data: FA 73  returns 0x02 (0000ms, 13542ms total)
T35A0 295:266 JLINK_ReadMemEx(0x08009F48, 0x003C Bytes, ..., Flags = 0x02000000) -- CPU_ReadMem(64 bytes @ 0x08009F80) -- Updating C cache (64 bytes @ 0x08009F80) -- Read from C cache (60 bytes @ 0x08009F48) - Data: 00 22 11 46 10 46 F9 F7 8D F8 40 21 05 48 F7 F7 ...  returns 0x3C (0004ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F48, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F48) - Data: 00 22  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4A) - Data: 11 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4A) - Data: 11 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F4C) - Data: 10 46 F9 F7 8D F8 40 21 05 48 F7 F7 81 FF 4F F4 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4C) - Data: 10 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F4C) - Data: 10 46 F9 F7 8D F8 40 21 05 48 F7 F7 81 FF 4F F4 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4C) - Data: 10 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4E) - Data: F9 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F4E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F4E) - Data: F9 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F50, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F50) - Data: 8D F8 40 21 05 48 F7 F7 81 FF 4F F4 FA 73 00 22 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F50, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F50) - Data: 8D F8  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F52, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F52) - Data: 40 21  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F54, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F54) - Data: 05 48 F7 F7 81 FF 4F F4 FA 73 00 22 11 46 10 46 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F54, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F54) - Data: 05 48  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F54, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F54) - Data: 05 48 F7 F7 81 FF 4F F4 FA 73 00 22 11 46 10 46 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F54, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F54) - Data: 05 48  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F56, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F56) - Data: F7 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F56, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F56) - Data: F7 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F58, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F58) - Data: 81 FF 4F F4 FA 73 00 22 11 46 10 46 F9 F7 82 F8 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F58, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F58) - Data: 81 FF  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F5A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F5A) - Data: 4F F4  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F5C, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F5C) - Data: FA 73 00 22 11 46 10 46 F9 F7 82 F8 E8 E7 00 00 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F5C, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F5C) - Data: FA 73  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F5E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F5E) - Data: 00 22  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F60, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F60) - Data: 11 46 10 46 F9 F7 82 F8 E8 E7 00 00 00 14 02 40 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F60, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F60) - Data: 11 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F60, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F60) - Data: 11 46 10 46 F9 F7 82 F8 E8 E7 00 00 00 14 02 40 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F60, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F60) - Data: 11 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F62, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F62) - Data: 10 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F62, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F62) - Data: 10 46  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F64, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F64) - Data: F9 F7 82 F8 E8 E7 00 00 00 14 02 40 FD F7 76 FD ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F64, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F64) - Data: F9 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F64, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F64) - Data: F9 F7 82 F8 E8 E7 00 00 00 14 02 40 FD F7 76 FD ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F64, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F64) - Data: F9 F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F66, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F66) - Data: 82 F8  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F68, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F68) - Data: E8 E7 00 00 00 14 02 40 FD F7 76 FD F8 F7 51 FB ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F68, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F68) - Data: E8 E7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F6A, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F6A) - Data: 00 00  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F6E, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F6E) - Data: 02 40  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F70, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F70) - Data: FD F7 76 FD F8 F7 51 FB 01 20 00 F0 4F FB 00 20 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F70, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F70) - Data: FD F7  returns 0x02 (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F70, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F70) - Data: FD F7 76 FD F8 F7 51 FB 01 20 00 F0 4F FB 00 20 ...  returns 0x3C (0000ms, 13546ms total)
T35A0 295:270 JLINK_ReadMemEx(0x08009F70, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F70) - Data: FD F7  returns 0x02 (0001ms, 13547ms total)
T35A0 295:271 JLINK_ReadMemEx(0x08009F72, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F72) - Data: 76 FD  returns 0x02 (0000ms, 13547ms total)
T35A0 295:271 JLINK_ReadMemEx(0x08009F74, 0x003C Bytes, ..., Flags = 0x02000000) -- Read from C cache (60 bytes @ 0x08009F74) - Data: F8 F7 51 FB 01 20 00 F0 4F FB 00 20 00 F0 4C FB ...  returns 0x3C (0000ms, 13547ms total)
T35A0 295:271 JLINK_ReadMemEx(0x08009F74, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F74) - Data: F8 F7  returns 0x02 (0000ms, 13547ms total)
T35A0 295:271 JLINK_ReadMemEx(0x08009F76, 0x0002 Bytes, ..., Flags = 0x02000000) -- Read from C cache (2 bytes @ 0x08009F76) - Data: 51 FB  returns 0x02 (0000ms, 13547ms total)
T35A0 565:742 JLINK_Close() -- CPU_WriteMem(4 bytes @ 0xE0002008) -- CPU_ReadMem(4 bytes @ 0xE0001000) -- CPU_WriteMem(4 bytes @ 0xE0001000)
  ***** Error: Could not start CPU core. (ErrorCode: -1) >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> >0x0D TIF> (0055ms, 13602ms total)
T35A0 565:742  (0055ms, 13602ms total)
T35A0 565:742 Closed (0055ms, 13602ms total)
